(kicad_pcb (version 20171130) (host pcbnew 5.1.9+dfsg1-1~bpo10+1)

  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 410)
    (zones 0)
    (modules 44)
    (nets 76)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.5 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 VCC)
  (net 7 "Net-(C6-Pad1)")
  (net 8 "Net-(D1-Pad1)")
  (net 9 "Net-(D1-Pad2)")
  (net 10 /IOEN0)
  (net 11 /IOEN1)
  (net 12 /IOEN2)
  (net 13 /IOEN3)
  (net 14 /IOEN4)
  (net 15 /IOEN5)
  (net 16 /IOEN6)
  (net 17 /IOEN7)
  (net 18 /IOADDR0)
  (net 19 /IOADDR1)
  (net 20 /IOADDR2)
  (net 21 /IOADDR3)
  (net 22 /IOADDR4)
  (net 23 /IOD0)
  (net 24 /IOD1)
  (net 25 /IOD2)
  (net 26 /IOD3)
  (net 27 /IOD4)
  (net 28 /IOD5)
  (net 29 /IOD6)
  (net 30 /IOD7)
  (net 31 /IOWR)
  (net 32 "Net-(J5-Pad1)")
  (net 33 "Net-(R3-Pad1)")
  (net 34 /A11)
  (net 35 /RD)
  (net 36 /A12)
  (net 37 /WR)
  (net 38 /A13)
  (net 39 "Net-(U1-Pad23)")
  (net 40 /A14)
  (net 41 /A15)
  (net 42 "Net-(U1-Pad6)")
  (net 43 "Net-(U1-Pad26)")
  (net 44 /D4)
  (net 45 "Net-(U1-Pad27)")
  (net 46 /D3)
  (net 47 "Net-(U1-Pad28)")
  (net 48 /D5)
  (net 49 /D6)
  (net 50 /A0)
  (net 51 /A1)
  (net 52 /D2)
  (net 53 /A2)
  (net 54 /D7)
  (net 55 /A3)
  (net 56 /D0)
  (net 57 /A4)
  (net 58 /D1)
  (net 59 /A5)
  (net 60 /A6)
  (net 61 /A7)
  (net 62 /A8)
  (net 63 "Net-(U1-Pad19)")
  (net 64 /A9)
  (net 65 /IORQ)
  (net 66 /A10)
  (net 67 /ROMEN)
  (net 68 /RAMEN)
  (net 69 "Net-(U10-Pad1)")
  (net 70 "Net-(U10-Pad2)")
  (net 71 "Net-(U11-Pad3)")
  (net 72 "Net-(U21-Pad18)")
  (net 73 "Net-(U21-Pad16)")
  (net 74 "Net-(U21-Pad4)")
  (net 75 "Net-(U21-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /IOADDR0)
    (add_net /IOADDR1)
    (add_net /IOADDR2)
    (add_net /IOADDR3)
    (add_net /IOADDR4)
    (add_net /IOD0)
    (add_net /IOD1)
    (add_net /IOD2)
    (add_net /IOD3)
    (add_net /IOD4)
    (add_net /IOD5)
    (add_net /IOD6)
    (add_net /IOD7)
    (add_net /IOEN0)
    (add_net /IOEN1)
    (add_net /IOEN2)
    (add_net /IOEN3)
    (add_net /IOEN4)
    (add_net /IOEN5)
    (add_net /IOEN6)
    (add_net /IOEN7)
    (add_net /IORQ)
    (add_net /IOWR)
    (add_net /RAMEN)
    (add_net /RD)
    (add_net /ROMEN)
    (add_net /WR)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U10-Pad1)")
    (add_net "Net-(U10-Pad2)")
    (add_net "Net-(U11-Pad3)")
    (add_net "Net-(U21-Pad16)")
    (add_net "Net-(U21-Pad18)")
    (add_net "Net-(U21-Pad2)")
    (add_net "Net-(U21-Pad4)")
    (add_net VCC)
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x26_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB) (tstamp 605C0224)
    (at 160.02 15.24)
    (descr "Through hole angled pin header, 1x26, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x26 2.54mm single row")
    (path /60940D54)
    (fp_text reference IOBUS1 (at 4.385 -2.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IO_bus_conn (at 4.385 65.77) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 10.55 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.55 65.3) (end 10.55 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 65.3) (end 10.55 65.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 65.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -1.27) (end 0 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 0) (end -1.27 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 63.88) (end 1.44 63.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 63.12) (end 1.44 63.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 63.88) (end 4.1 63.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 63.12) (end 10.1 63.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 63.12) (end 10.1 63.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 62.23) (end 4.1 62.23) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 61.34) (end 1.44 61.34) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 60.58) (end 1.44 60.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 61.34) (end 4.1 61.34) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 60.58) (end 10.1 61.34) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 60.58) (end 10.1 60.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 59.69) (end 4.1 59.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 58.8) (end 1.44 58.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 58.04) (end 1.44 58.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 58.8) (end 4.1 58.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 58.04) (end 10.1 58.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 58.04) (end 10.1 58.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 57.15) (end 4.1 57.15) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 56.26) (end 1.44 56.26) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 55.5) (end 1.44 55.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 56.26) (end 4.1 56.26) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 55.5) (end 10.1 56.26) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 55.5) (end 10.1 55.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 54.61) (end 4.1 54.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 53.72) (end 1.44 53.72) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 52.96) (end 1.44 52.96) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 53.72) (end 4.1 53.72) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 52.96) (end 10.1 53.72) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 52.96) (end 10.1 52.96) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 52.07) (end 4.1 52.07) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 51.18) (end 1.44 51.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 50.42) (end 1.44 50.42) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 51.18) (end 4.1 51.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 50.42) (end 10.1 51.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 50.42) (end 10.1 50.42) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 49.53) (end 4.1 49.53) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 48.64) (end 1.44 48.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 47.88) (end 1.44 47.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 48.64) (end 4.1 48.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 47.88) (end 10.1 48.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 47.88) (end 10.1 47.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 46.99) (end 4.1 46.99) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 46.1) (end 1.44 46.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 45.34) (end 1.44 45.34) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 46.1) (end 4.1 46.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 45.34) (end 10.1 46.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 45.34) (end 10.1 45.34) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 44.45) (end 4.1 44.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 43.56) (end 1.44 43.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 42.8) (end 1.44 42.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 43.56) (end 4.1 43.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 42.8) (end 10.1 43.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 42.8) (end 10.1 42.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 41.91) (end 4.1 41.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 41.02) (end 1.44 41.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 40.26) (end 1.44 40.26) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 41.02) (end 4.1 41.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 40.26) (end 10.1 41.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 40.26) (end 10.1 40.26) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 39.37) (end 4.1 39.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 38.48) (end 1.44 38.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 37.72) (end 1.44 37.72) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 38.48) (end 4.1 38.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 37.72) (end 10.1 38.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 37.72) (end 10.1 37.72) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 36.83) (end 4.1 36.83) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 35.94) (end 1.44 35.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 35.18) (end 1.44 35.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 35.94) (end 4.1 35.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 35.18) (end 10.1 35.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 35.18) (end 10.1 35.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 34.29) (end 4.1 34.29) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 33.4) (end 1.44 33.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 32.64) (end 1.44 32.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 33.4) (end 4.1 33.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 32.64) (end 10.1 33.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 32.64) (end 10.1 32.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 31.75) (end 4.1 31.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 30.86) (end 1.44 30.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 30.1) (end 1.44 30.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 30.86) (end 4.1 30.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 30.1) (end 10.1 30.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 30.1) (end 10.1 30.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 29.21) (end 4.1 29.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 28.32) (end 1.44 28.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 27.56) (end 1.44 27.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 28.32) (end 4.1 28.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 27.56) (end 10.1 28.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 27.56) (end 10.1 27.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 26.67) (end 4.1 26.67) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 25.78) (end 1.44 25.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 25.02) (end 1.44 25.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 25.78) (end 4.1 25.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 25.02) (end 10.1 25.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 25.02) (end 10.1 25.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 24.13) (end 4.1 24.13) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 23.24) (end 1.44 23.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 22.48) (end 1.44 22.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 23.24) (end 4.1 23.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 22.48) (end 10.1 23.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 22.48) (end 10.1 22.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 21.59) (end 4.1 21.59) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 20.7) (end 1.44 20.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 19.94) (end 1.44 19.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 20.7) (end 4.1 20.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 19.94) (end 10.1 20.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 19.94) (end 10.1 19.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 19.05) (end 4.1 19.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 18.16) (end 1.44 18.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 17.4) (end 1.44 17.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 18.16) (end 4.1 18.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 17.4) (end 10.1 18.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 17.4) (end 10.1 17.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 16.51) (end 4.1 16.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 15.62) (end 1.44 15.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 14.86) (end 1.44 14.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 15.62) (end 4.1 15.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 14.86) (end 10.1 15.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 14.86) (end 10.1 14.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 13.97) (end 4.1 13.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 13.08) (end 1.44 13.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 12.32) (end 1.44 12.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 13.08) (end 4.1 13.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 12.32) (end 10.1 13.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 12.32) (end 10.1 12.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 11.43) (end 4.1 11.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 10.54) (end 1.44 10.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 9.78) (end 1.44 9.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 10.54) (end 4.1 10.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 9.78) (end 10.1 10.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 9.78) (end 10.1 9.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 8.89) (end 4.1 8.89) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 8) (end 1.44 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 7.24) (end 1.44 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 8) (end 4.1 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 7.24) (end 10.1 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 7.24) (end 10.1 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 6.35) (end 4.1 6.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 5.46) (end 1.44 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 4.7) (end 1.44 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 5.46) (end 4.1 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 4.7) (end 10.1 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 4.7) (end 10.1 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 3.81) (end 4.1 3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.92) (end 1.44 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.16) (end 1.44 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 2.92) (end 4.1 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 2.16) (end 10.1 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 2.16) (end 10.1 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 1.27) (end 4.1 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.38) (end 1.44 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 -0.38) (end 1.44 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.28) (end 10.1 0.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.16) (end 10.1 0.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.04) (end 10.1 0.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.08) (end 10.1 -0.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.2) (end 10.1 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.32) (end 10.1 -0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 0.38) (end 4.1 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 -0.38) (end 10.1 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.38) (end 10.1 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -1.33) (end 1.44 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 64.83) (end 4.1 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 64.83) (end 4.1 64.83) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 -1.33) (end 1.44 64.83) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.04 63.82) (end 10.04 63.82) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 63.18) (end 10.04 63.82) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 63.18) (end 10.04 63.18) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 63.82) (end 1.5 63.82) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 63.18) (end -0.32 63.82) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 63.18) (end 1.5 63.18) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 61.28) (end 10.04 61.28) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 60.64) (end 10.04 61.28) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 60.64) (end 10.04 60.64) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 61.28) (end 1.5 61.28) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 60.64) (end -0.32 61.28) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 60.64) (end 1.5 60.64) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 58.74) (end 10.04 58.74) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 58.1) (end 10.04 58.74) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 58.1) (end 10.04 58.1) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 58.74) (end 1.5 58.74) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 58.1) (end -0.32 58.74) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 58.1) (end 1.5 58.1) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 56.2) (end 10.04 56.2) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 55.56) (end 10.04 56.2) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 55.56) (end 10.04 55.56) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 56.2) (end 1.5 56.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 55.56) (end -0.32 56.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 55.56) (end 1.5 55.56) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 53.66) (end 10.04 53.66) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 53.02) (end 10.04 53.66) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 53.02) (end 10.04 53.02) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 53.66) (end 1.5 53.66) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 53.02) (end -0.32 53.66) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 53.02) (end 1.5 53.02) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 51.12) (end 10.04 51.12) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 50.48) (end 10.04 51.12) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 50.48) (end 10.04 50.48) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 51.12) (end 1.5 51.12) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 50.48) (end -0.32 51.12) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 50.48) (end 1.5 50.48) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 48.58) (end 10.04 48.58) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 47.94) (end 10.04 48.58) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 47.94) (end 10.04 47.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 48.58) (end 1.5 48.58) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 47.94) (end -0.32 48.58) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 47.94) (end 1.5 47.94) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 46.04) (end 10.04 46.04) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 45.4) (end 10.04 46.04) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 45.4) (end 10.04 45.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 46.04) (end 1.5 46.04) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 45.4) (end -0.32 46.04) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 45.4) (end 1.5 45.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 43.5) (end 10.04 43.5) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 42.86) (end 10.04 43.5) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 42.86) (end 10.04 42.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 43.5) (end 1.5 43.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 42.86) (end -0.32 43.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 42.86) (end 1.5 42.86) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 40.96) (end 10.04 40.96) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 40.32) (end 10.04 40.96) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 40.32) (end 10.04 40.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 40.96) (end 1.5 40.96) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 40.32) (end -0.32 40.96) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 40.32) (end 1.5 40.32) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 38.42) (end 10.04 38.42) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 37.78) (end 10.04 38.42) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 37.78) (end 10.04 37.78) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 38.42) (end 1.5 38.42) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 37.78) (end -0.32 38.42) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 37.78) (end 1.5 37.78) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 35.88) (end 10.04 35.88) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 35.24) (end 10.04 35.88) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 35.24) (end 10.04 35.24) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 35.88) (end 1.5 35.88) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 35.24) (end -0.32 35.88) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 35.24) (end 1.5 35.24) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 33.34) (end 10.04 33.34) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 32.7) (end 10.04 33.34) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 32.7) (end 10.04 32.7) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 33.34) (end 1.5 33.34) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 32.7) (end -0.32 33.34) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 32.7) (end 1.5 32.7) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 30.8) (end 10.04 30.8) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 30.16) (end 10.04 30.8) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 30.16) (end 10.04 30.16) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 30.8) (end 1.5 30.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 30.16) (end -0.32 30.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 30.16) (end 1.5 30.16) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 28.26) (end 10.04 28.26) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 27.62) (end 10.04 28.26) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 27.62) (end 10.04 27.62) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 28.26) (end 1.5 28.26) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 27.62) (end -0.32 28.26) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 27.62) (end 1.5 27.62) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 25.72) (end 10.04 25.72) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 25.08) (end 10.04 25.72) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 25.08) (end 10.04 25.08) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 25.72) (end 1.5 25.72) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 25.08) (end -0.32 25.72) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 25.08) (end 1.5 25.08) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 23.18) (end 10.04 23.18) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 22.54) (end 10.04 23.18) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 22.54) (end 10.04 22.54) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 23.18) (end 1.5 23.18) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 22.54) (end -0.32 23.18) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 22.54) (end 1.5 22.54) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 20.64) (end 10.04 20.64) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 20) (end 10.04 20.64) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 20) (end 10.04 20) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 20.64) (end 1.5 20.64) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 20) (end -0.32 20.64) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 20) (end 1.5 20) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 18.1) (end 10.04 18.1) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 17.46) (end 10.04 18.1) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 17.46) (end 10.04 17.46) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 18.1) (end 1.5 18.1) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 17.46) (end -0.32 18.1) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 17.46) (end 1.5 17.46) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 15.56) (end 10.04 15.56) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 14.92) (end 10.04 15.56) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 14.92) (end 10.04 14.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 15.56) (end 1.5 15.56) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 14.92) (end -0.32 15.56) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 14.92) (end 1.5 14.92) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 13.02) (end 10.04 13.02) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 12.38) (end 10.04 13.02) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 12.38) (end 10.04 12.38) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 13.02) (end 1.5 13.02) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 12.38) (end -0.32 13.02) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 12.38) (end 1.5 12.38) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 10.48) (end 10.04 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 9.84) (end 10.04 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 9.84) (end 10.04 9.84) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 10.48) (end 1.5 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 9.84) (end -0.32 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 9.84) (end 1.5 9.84) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 7.94) (end 10.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 7.3) (end 10.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 7.3) (end 10.04 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.94) (end 1.5 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end -0.32 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end 1.5 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 5.4) (end 10.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 4.76) (end 10.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 4.76) (end 10.04 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 5.4) (end 1.5 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end -0.32 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end 1.5 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 2.86) (end 10.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 2.22) (end 10.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 2.22) (end 10.04 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.86) (end 1.5 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end -0.32 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end 1.5 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 -0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -0.32) (end 10.04 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 0.32) (end 1.5 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end -0.32 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end 1.5 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -0.635) (end 2.135 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 64.77) (end 1.5 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 64.77) (end 1.5 64.77) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -1.27) (end 4.04 64.77) (layer F.Fab) (width 0.1))
    (fp_line (start 2.135 -1.27) (end 4.04 -1.27) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.77 31.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /IOEN0))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /IOEN1))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /IOEN2))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /IOEN3))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /IOEN4))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /IOEN5))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /IOEN6))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /IOEN7))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /IOADDR0))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /IOADDR1))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /IOADDR2))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /IOADDR3))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /IOADDR4))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /IOD0))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /IOD1))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /IOD2))
    (pad 19 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /IOD3))
    (pad 20 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /IOD4))
    (pad 21 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /IOD5))
    (pad 22 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /IOD6))
    (pad 23 thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /IOD7))
    (pad 24 thru_hole oval (at 0 58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /IOWR))
    (pad 25 thru_hole oval (at 0 60.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at 0 63.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x26_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BDA87)
    (at 53.34 95.25 270)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /605648D0)
    (fp_text reference C2 (at 2.5 -4.25 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 30pF (at 2.5 4.25 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BF0A3)
    (at 60.96 95.25 270)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /60567676)
    (fp_text reference C3 (at 2.5 -4.25 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 30pF (at 2.5 4.25 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BB135)
    (at 302.465001 180.725001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /6068233C)
    (fp_text reference C1 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10uF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BB162)
    (at 310.955001 189.215001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /60B9FCED)
    (fp_text reference C4 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0,22uF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BB171)
    (at 298.105001 197.705001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /60BB291F)
    (fp_text reference C5 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0,1uF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BDA1B)
    (at 282.805001 211.065001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /6052B4C4)
    (fp_text reference C6 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10uF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BD8E7)
    (at 283.870242 219.235001)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (path /60AC0A76)
    (fp_text reference C7 (at 1.25 -4.4) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 1.25 4.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.935241 -2.154) (end -1.935241 -1.524) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.250241 -1.839) (end -1.620241 -1.839) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.491 -0.402) (end 4.491 0.402) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.451 -0.633) (end 4.451 0.633) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.411 -0.802) (end 4.411 0.802) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.371 -0.94) (end 4.371 0.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.331 -1.059) (end 4.331 1.059) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.291 -1.165) (end 4.291 1.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.251 -1.262) (end 4.251 1.262) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.211 -1.35) (end 4.211 1.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.171 -1.432) (end 4.171 1.432) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.131 -1.509) (end 4.131 1.509) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.091 -1.581) (end 4.091 1.581) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.051 -1.65) (end 4.051 1.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.011 -1.714) (end 4.011 1.714) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.971 -1.776) (end 3.971 1.776) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.931 -1.834) (end 3.931 1.834) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.891 -1.89) (end 3.891 1.89) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.851 -1.944) (end 3.851 1.944) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -1.995) (end 3.811 1.995) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -2.044) (end 3.771 2.044) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -2.092) (end 3.731 2.092) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -2.137) (end 3.691 2.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -2.182) (end 3.651 2.182) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -2.224) (end 3.611 2.224) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -2.265) (end 3.571 2.265) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 1.04) (end 3.531 2.305) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -2.305) (end 3.531 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 1.04) (end 3.491 2.343) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -2.343) (end 3.491 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 1.04) (end 3.451 2.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -2.38) (end 3.451 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 1.04) (end 3.411 2.416) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -2.416) (end 3.411 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 1.04) (end 3.371 2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -2.45) (end 3.371 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 1.04) (end 3.331 2.484) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -2.484) (end 3.331 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 1.04) (end 3.291 2.516) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -2.516) (end 3.291 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 1.04) (end 3.251 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -2.548) (end 3.251 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 1.04) (end 3.211 2.578) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -2.578) (end 3.211 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 1.04) (end 3.171 2.607) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -2.607) (end 3.171 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 1.04) (end 3.131 2.636) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -2.636) (end 3.131 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 1.04) (end 3.091 2.664) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -2.664) (end 3.091 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 1.04) (end 3.051 2.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -2.69) (end 3.051 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 1.04) (end 3.011 2.716) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -2.716) (end 3.011 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 1.04) (end 2.971 2.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -2.742) (end 2.971 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 1.04) (end 2.931 2.766) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -2.766) (end 2.931 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 1.04) (end 2.891 2.79) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -2.79) (end 2.891 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 1.04) (end 2.851 2.812) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -2.812) (end 2.851 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 1.04) (end 2.811 2.834) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.834) (end 2.811 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 1.04) (end 2.771 2.856) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.856) (end 2.771 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 1.04) (end 2.731 2.876) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.876) (end 2.731 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 1.04) (end 2.691 2.896) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.896) (end 2.691 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 1.04) (end 2.651 2.916) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.916) (end 2.651 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 1.04) (end 2.611 2.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.934) (end 2.611 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 1.04) (end 2.571 2.952) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.952) (end 2.571 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 1.04) (end 2.531 2.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.97) (end 2.531 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 1.04) (end 2.491 2.986) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.986) (end 2.491 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 1.04) (end 2.451 3.002) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -3.002) (end 2.451 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 1.04) (end 2.411 3.018) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -3.018) (end 2.411 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 1.04) (end 2.371 3.033) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -3.033) (end 2.371 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 1.04) (end 2.331 3.047) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -3.047) (end 2.331 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 1.04) (end 2.291 3.061) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -3.061) (end 2.291 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 1.04) (end 2.251 3.074) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -3.074) (end 2.251 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 1.04) (end 2.211 3.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -3.086) (end 2.211 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 1.04) (end 2.171 3.098) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -3.098) (end 2.171 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 1.04) (end 2.131 3.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -3.11) (end 2.131 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 1.04) (end 2.091 3.121) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -3.121) (end 2.091 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 1.04) (end 2.051 3.131) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -3.131) (end 2.051 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 1.04) (end 2.011 3.141) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -3.141) (end 2.011 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 1.04) (end 1.971 3.15) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -3.15) (end 1.971 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 1.04) (end 1.93 3.159) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -3.159) (end 1.93 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 1.04) (end 1.89 3.167) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -3.167) (end 1.89 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 1.04) (end 1.85 3.175) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -3.175) (end 1.85 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.04) (end 1.81 3.182) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -3.182) (end 1.81 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 1.04) (end 1.77 3.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -3.189) (end 1.77 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 1.04) (end 1.73 3.195) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -3.195) (end 1.73 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 1.04) (end 1.69 3.201) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -3.201) (end 1.69 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 1.04) (end 1.65 3.206) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -3.206) (end 1.65 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 1.04) (end 1.61 3.211) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -3.211) (end 1.61 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 1.04) (end 1.57 3.215) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -3.215) (end 1.57 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 1.04) (end 1.53 3.218) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -3.218) (end 1.53 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 1.04) (end 1.49 3.222) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -3.222) (end 1.49 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -3.224) (end 1.45 3.224) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -3.227) (end 1.41 3.227) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -3.228) (end 1.37 3.228) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -3.23) (end 1.33 3.23) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -3.23) (end 1.29 3.23) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.25 -3.23) (end 1.25 3.23) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.128972 -1.6885) (end -1.128972 -1.0585) (layer F.Fab) (width 0.1))
    (fp_line (start -1.443972 -1.3735) (end -0.813972 -1.3735) (layer F.Fab) (width 0.1))
    (fp_circle (center 1.25 0) (end 4.65 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 1.25 0) (end 4.52 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 4.4 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BD838)
    (at 274.315001 220.015001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /6055A1F9)
    (fp_text reference C8 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BB232)
    (at 281.125001 187.325001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /6055A9DD)
    (fp_text reference C9 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 56pF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BB241)
    (at 316.375001 161.225001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /606345B4)
    (fp_text reference C10 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 56pF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BB250)
    (at 140.349001 190.189001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /606345AE)
    (fp_text reference C11 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BD80E)
    (at 284.885001 202.575001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /60649CAE)
    (fp_text reference C12 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 56pF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BB26E)
    (at 289.615001 192.225001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /60649CA8)
    (fp_text reference C13 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BD7E4)
    (at 276.395001 202.575001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /6062D6ED)
    (fp_text reference C14 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BD7BA)
    (at 274.315001 211.525001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /6062D6F3)
    (fp_text reference C15 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 56pF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BB29B)
    (at 310.955001 180.725001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /60853D7B)
    (fp_text reference C16 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BB2AA)
    (at 302.465001 189.215001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /60853D81)
    (fp_text reference C17 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 56pF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BB2B9)
    (at 316.375001 169.715001)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /6084DC4D)
    (fp_text reference C18 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BB2C8)
    (at 154.94 177.8)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (path /6084DC53)
    (fp_text reference C19 (at 2.5 -4.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 56pF (at 2.5 4.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.539749 -2.055) (end -0.539749 -1.455) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.839749 -1.755) (end -0.239749 -1.755) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.235344 -1.6075) (end 0.235344 -1.0075) (layer F.Fab) (width 0.1))
    (fp_line (start -0.064656 -1.3075) (end 0.535344 -1.3075) (layer F.Fab) (width 0.1))
    (fp_circle (center 2.5 0) (end 6.22 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.5 0) (end 5.5 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.5 0) (end -0.434416 -1.06) (angle 140.277494) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.5 0) (end -0.434416 1.06) (angle -140.277494) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 605BB35C)
    (at 307.660242 197.385001)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (path /60AED147)
    (fp_text reference C20 (at 1.25 -4.4) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 1.25 4.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 1.25 0) (end 4.4 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 1.25 0) (end 4.52 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 4.65 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.443972 -1.3735) (end -0.813972 -1.3735) (layer F.Fab) (width 0.1))
    (fp_line (start -1.128972 -1.6885) (end -1.128972 -1.0585) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -3.23) (end 1.25 3.23) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -3.23) (end 1.29 3.23) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -3.23) (end 1.33 3.23) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -3.228) (end 1.37 3.228) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -3.227) (end 1.41 3.227) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -3.224) (end 1.45 3.224) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -3.222) (end 1.49 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 1.04) (end 1.49 3.222) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -3.218) (end 1.53 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 1.04) (end 1.53 3.218) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -3.215) (end 1.57 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 1.04) (end 1.57 3.215) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -3.211) (end 1.61 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 1.04) (end 1.61 3.211) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -3.206) (end 1.65 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 1.04) (end 1.65 3.206) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -3.201) (end 1.69 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 1.04) (end 1.69 3.201) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -3.195) (end 1.73 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 1.04) (end 1.73 3.195) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -3.189) (end 1.77 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 1.04) (end 1.77 3.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -3.182) (end 1.81 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 1.04) (end 1.81 3.182) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -3.175) (end 1.85 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 1.04) (end 1.85 3.175) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -3.167) (end 1.89 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 1.04) (end 1.89 3.167) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -3.159) (end 1.93 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 1.04) (end 1.93 3.159) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -3.15) (end 1.971 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 1.04) (end 1.971 3.15) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -3.141) (end 2.011 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 1.04) (end 2.011 3.141) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -3.131) (end 2.051 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 1.04) (end 2.051 3.131) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -3.121) (end 2.091 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 1.04) (end 2.091 3.121) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -3.11) (end 2.131 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 1.04) (end 2.131 3.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -3.098) (end 2.171 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 1.04) (end 2.171 3.098) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -3.086) (end 2.211 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 1.04) (end 2.211 3.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -3.074) (end 2.251 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 1.04) (end 2.251 3.074) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -3.061) (end 2.291 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 1.04) (end 2.291 3.061) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -3.047) (end 2.331 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 1.04) (end 2.331 3.047) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -3.033) (end 2.371 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 1.04) (end 2.371 3.033) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -3.018) (end 2.411 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 1.04) (end 2.411 3.018) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -3.002) (end 2.451 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 1.04) (end 2.451 3.002) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.986) (end 2.491 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 1.04) (end 2.491 2.986) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.97) (end 2.531 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 1.04) (end 2.531 2.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.952) (end 2.571 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 1.04) (end 2.571 2.952) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.934) (end 2.611 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 1.04) (end 2.611 2.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.916) (end 2.651 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 1.04) (end 2.651 2.916) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.896) (end 2.691 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 1.04) (end 2.691 2.896) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.876) (end 2.731 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 1.04) (end 2.731 2.876) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.856) (end 2.771 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 1.04) (end 2.771 2.856) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.834) (end 2.811 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 1.04) (end 2.811 2.834) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -2.812) (end 2.851 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 1.04) (end 2.851 2.812) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -2.79) (end 2.891 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 1.04) (end 2.891 2.79) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -2.766) (end 2.931 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 1.04) (end 2.931 2.766) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -2.742) (end 2.971 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 1.04) (end 2.971 2.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -2.716) (end 3.011 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 1.04) (end 3.011 2.716) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -2.69) (end 3.051 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 1.04) (end 3.051 2.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -2.664) (end 3.091 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 1.04) (end 3.091 2.664) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -2.636) (end 3.131 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 1.04) (end 3.131 2.636) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -2.607) (end 3.171 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 1.04) (end 3.171 2.607) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -2.578) (end 3.211 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 1.04) (end 3.211 2.578) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -2.548) (end 3.251 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 1.04) (end 3.251 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -2.516) (end 3.291 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 1.04) (end 3.291 2.516) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -2.484) (end 3.331 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 1.04) (end 3.331 2.484) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -2.45) (end 3.371 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 1.04) (end 3.371 2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -2.416) (end 3.411 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 1.04) (end 3.411 2.416) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -2.38) (end 3.451 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 1.04) (end 3.451 2.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -2.343) (end 3.491 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 1.04) (end 3.491 2.343) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -2.305) (end 3.531 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 1.04) (end 3.531 2.305) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -2.265) (end 3.571 2.265) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -2.224) (end 3.611 2.224) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -2.182) (end 3.651 2.182) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -2.137) (end 3.691 2.137) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -2.092) (end 3.731 2.092) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -2.044) (end 3.771 2.044) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -1.995) (end 3.811 1.995) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.851 -1.944) (end 3.851 1.944) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.891 -1.89) (end 3.891 1.89) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.931 -1.834) (end 3.931 1.834) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.971 -1.776) (end 3.971 1.776) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.011 -1.714) (end 4.011 1.714) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.051 -1.65) (end 4.051 1.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.091 -1.581) (end 4.091 1.581) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.131 -1.509) (end 4.131 1.509) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.171 -1.432) (end 4.171 1.432) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.211 -1.35) (end 4.211 1.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.251 -1.262) (end 4.251 1.262) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.291 -1.165) (end 4.291 1.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.331 -1.059) (end 4.331 1.059) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.371 -0.94) (end 4.371 0.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.411 -0.802) (end 4.411 0.802) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.451 -0.633) (end 4.451 0.633) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.491 -0.402) (end 4.491 0.402) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.250241 -1.839) (end -1.620241 -1.839) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.935241 -2.154) (end -1.935241 -1.524) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A) (tstamp 605BB36E)
    (at 320.175001 186.225001)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (path /606D4ECC)
    (fp_text reference D1 (at 1.27 -3.96) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 1.27 3.96) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.5 -3.25) (end -1.95 -3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 3.25) (end 4.5 -3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 3.25) (end 4.5 3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -3.25) (end -1.95 3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.29 -1.545) (end -1.29 1.545) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.23 -1.469694) (end -1.23 1.469694) (layer F.Fab) (width 0.1))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end -1.23 -1.469694) (angle 299.1) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end -1.29 -1.54483) (angle 148.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -1.29 1.54483) (angle -148.9) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 1.25 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.2)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 605BB4EE)
    (at 109.579001 197.669001)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (path /606C1179)
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value panel_btn_brk (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.33) (end 1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 605BB504)
    (at 109.22 185.42)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (path /60AE4278)
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Power input" (at 0 4.87) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 605BD784)
    (at 293.955001 198.795001)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (path /60701566)
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value panel_led_halt (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.33) (end 1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 605BB52E)
    (at 325.445001 163.955001)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (path /606A5B44)
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value panel_btn_rst (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 1.33) (end 1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 605BB543)
    (at 325.445001 159.305001)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (path /60B92792)
    (fp_text reference J5 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value nmi (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 1.33) (end 1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 605BF0D5)
    (at 53.34 91.44)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /60581F4C)
    (fp_text reference R1 (at 3.81 -2.37) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3,3M (at 3.81 2.37) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.54 -1.04) (end 0.54 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 -1.37) (end 7.08 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.08 -1.37) (end 7.08 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 1.04) (end 0.54 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 1.37) (end 7.08 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.08 1.37) (end 7.08 1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 8.67 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.67 1.5) (end 8.67 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.67 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 605BB571)
    (at 121.92 182.88)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /60662809)
    (fp_text reference R2 (at 3.81 -2.37) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 2.37) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.54 -1.04) (end 0.54 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 -1.37) (end 7.08 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.08 -1.37) (end 7.08 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 1.04) (end 0.54 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 1.37) (end 7.08 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.08 1.37) (end 7.08 1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 8.67 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.67 1.5) (end 8.67 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.67 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 605BB588)
    (at 140.179001 174.969001)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /60661B57)
    (fp_text reference R3 (at 3.81 -2.37) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 2.37) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.67 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.67 1.5) (end 8.67 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 8.67 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.08 1.37) (end 7.08 1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 1.37) (end 7.08 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 1.04) (end 0.54 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.08 -1.37) (end 7.08 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 -1.37) (end 7.08 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 -1.04) (end 0.54 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 605BB59F)
    (at 280.955001 181.055001)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /606E9AF9)
    (fp_text reference R4 (at 3.81 -2.37) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470 (at 3.81 2.37) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.67 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.67 1.5) (end 8.67 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 8.67 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.08 1.37) (end 7.08 1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 1.37) (end 7.08 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 1.04) (end 0.54 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.08 -1.37) (end 7.08 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 -1.37) (end 7.08 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 -1.04) (end 0.54 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 605BB5B6)
    (at 108.829001 202.069001)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /60584118)
    (fp_text reference R5 (at 3.81 -2.37) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 270k (at 3.81 2.37) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.67 -1.5) (end -1.05 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.67 1.5) (end 8.67 -1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.5) (end 8.67 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.08 1.37) (end 7.08 1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 1.37) (end 7.08 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 1.04) (end 0.54 1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.08 -1.37) (end 7.08 -1.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 -1.37) (end 7.08 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.54 -1.04) (end 0.54 -1.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 6.96 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0.66 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 -1.25) (end 0.66 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 6.96 1.25) (end 6.96 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 1.25) (end 6.96 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.66 -1.25) (end 0.66 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Button_Switch_THT:SW_Tactile_Straight_KSA0Axx1LFTR (layer F.Cu) (tedit 5A02FE31) (tstamp 605BB5D0)
    (at 140.079001 178.929001)
    (descr "SW PUSH SMALL http://www.ckswitches.com/media/1457/ksa_ksl.pdf")
    (tags "SW PUSH SMALL Tactile C&K")
    (path /60528DA4)
    (fp_text reference SW1 (at 3.81 -2.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 3.81 7.28) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 3.81 2.54) (end 3.81 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 6.05) (end 0 6.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 6.05) (end 7.62 6.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.57 6.49) (end -0.95 6.49) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 6.49) (end 8.57 -1.41) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.41) (end -0.95 6.49) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.41) (end 8.57 -1.41) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0 0.97) (end 0 4.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0.97) (end 7.62 4.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -1.27) (end 0 -0.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 6.35) (end 0 6.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 -1.27) (end 7.62 -0.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.11 6.24) (end 0.11 -1.16) (layer F.Fab) (width 0.1))
    (fp_line (start 0.11 -1.16) (end 7.51 -1.16) (layer F.Fab) (width 0.1))
    (fp_line (start 7.51 -1.16) (end 7.51 6.24) (layer F.Fab) (width 0.1))
    (fp_line (start 7.51 6.24) (end 0.11 6.24) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 3.81 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 7.62 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 7.62 5.08) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 5.08) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_Tactile_Straight_KSA0Axx1LFTR.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Button_Switch_THT:SW_Tactile_Straight_KSA0Axx1LFTR (layer F.Cu) (tedit 5A02FE31) (tstamp 605BB5EA)
    (at 291.625001 180.965001)
    (descr "SW PUSH SMALL http://www.ckswitches.com/media/1457/ksa_ksl.pdf")
    (tags "SW PUSH SMALL Tactile C&K")
    (path /6067F418)
    (fp_text reference SW2 (at 3.81 -2.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Break (at 3.81 7.28) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 2.54) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.51 6.24) (end 0.11 6.24) (layer F.Fab) (width 0.1))
    (fp_line (start 7.51 -1.16) (end 7.51 6.24) (layer F.Fab) (width 0.1))
    (fp_line (start 0.11 -1.16) (end 7.51 -1.16) (layer F.Fab) (width 0.1))
    (fp_line (start 0.11 6.24) (end 0.11 -1.16) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -1.27) (end 7.62 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 -1.27) (end 7.62 -0.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 6.35) (end 0 6.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -1.27) (end 0 -0.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0.97) (end 7.62 4.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 0.97) (end 0 4.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.41) (end 8.57 -1.41) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.41) (end -0.95 6.49) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 6.49) (end 8.57 -1.41) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 6.49) (end -0.95 6.49) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.62 6.05) (end 7.62 6.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 6.05) (end 0 6.35) (layer F.SilkS) (width 0.12))
    (fp_circle (center 3.81 2.54) (end 3.81 0) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 0 5.08) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 7.62 5.08) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 7.62 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_Tactile_Straight_KSA0Axx1LFTR.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-40_W15.24mm_Socket_LongPads (layer F.Cu) (tedit 5A02E8C5) (tstamp 605BB62E)
    (at 86.36 17.78)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads")
    (path /604F040E)
    (fp_text reference U1 (at 7.62 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Z80CPU (at 7.62 50.59) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 16.8 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.8 49.85) (end 16.8 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 49.85) (end 16.8 49.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -1.6) (end -1.55 49.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.68 -1.39) (end -1.44 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.68 49.65) (end 16.68 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 49.65) (end 16.68 49.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 -1.39) (end -1.44 49.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.68 -1.33) (end 8.62 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.68 49.59) (end 13.68 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 49.59) (end 13.68 49.59) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -1.33) (end 1.56 49.59) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.62 -1.33) (end 1.56 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.51 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 16.51 49.59) (end 16.51 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 49.59) (end 16.51 49.59) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.33) (end -1.27 49.59) (layer F.Fab) (width 0.1))
    (fp_line (start 0.255 -0.27) (end 1.255 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.255 49.53) (end 0.255 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 14.985 49.53) (end 0.255 49.53) (layer F.Fab) (width 0.1))
    (fp_line (start 14.985 -1.27) (end 14.985 49.53) (layer F.Fab) (width 0.1))
    (fp_line (start 1.255 -1.27) (end 14.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_arc (start 7.62 -1.33) (end 6.62 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 7.62 24.13) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /A11))
    (pad 21 thru_hole oval (at 15.24 48.26) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /RD))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /A12))
    (pad 22 thru_hole oval (at 15.24 45.72) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /WR))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /A13))
    (pad 23 thru_hole oval (at 15.24 43.18) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad23)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /A14))
    (pad 24 thru_hole oval (at 15.24 40.64) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /A15))
    (pad 25 thru_hole oval (at 15.24 38.1) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad6)"))
    (pad 26 thru_hole oval (at 15.24 35.56) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad26)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /D4))
    (pad 27 thru_hole oval (at 15.24 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U1-Pad27)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /D3))
    (pad 28 thru_hole oval (at 15.24 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U1-Pad28)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /D5))
    (pad 29 thru_hole oval (at 15.24 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /D6))
    (pad 30 thru_hole oval (at 15.24 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /A0))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 31 thru_hole oval (at 15.24 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /A1))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /D2))
    (pad 32 thru_hole oval (at 15.24 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /A2))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /D7))
    (pad 33 thru_hole oval (at 15.24 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /A3))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /D0))
    (pad 34 thru_hole oval (at 15.24 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /A4))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /D1))
    (pad 35 thru_hole oval (at 15.24 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 /A5))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 36 thru_hole oval (at 15.24 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /A6))
    (pad 17 thru_hole oval (at 0 40.64) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R3-Pad1)"))
    (pad 37 thru_hole oval (at 15.24 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 /A7))
    (pad 18 thru_hole oval (at 0 43.18) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (pad 38 thru_hole oval (at 15.24 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /A8))
    (pad 19 thru_hole oval (at 0 45.72) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(U1-Pad19)"))
    (pad 39 thru_hole oval (at 15.24 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /A9))
    (pad 20 thru_hole oval (at 0 48.26) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /IORQ))
    (pad 40 thru_hole oval (at 15.24 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /A10))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-40_W15.24mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-28_W15.24mm_Socket_LongPads (layer F.Cu) (tedit 5A02E8C5) (tstamp 605BB666)
    (at 53.34 17.78)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads")
    (path /604F6B81)
    (fp_text reference U2 (at 7.62 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "256k (32k x 8) EEPROM" (at 7.62 35.35) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 7.62 16.51) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 7.62 -1.33) (end 6.62 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.255 -1.27) (end 14.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 14.985 -1.27) (end 14.985 34.29) (layer F.Fab) (width 0.1))
    (fp_line (start 14.985 34.29) (end 0.255 34.29) (layer F.Fab) (width 0.1))
    (fp_line (start 0.255 34.29) (end 0.255 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.255 -0.27) (end 1.255 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.33) (end -1.27 34.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 34.35) (end 16.51 34.35) (layer F.Fab) (width 0.1))
    (fp_line (start 16.51 34.35) (end 16.51 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 16.51 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 6.62 -1.33) (end 1.56 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -1.33) (end 1.56 34.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 34.35) (end 13.68 34.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.68 34.35) (end 13.68 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.68 -1.33) (end 8.62 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 -1.39) (end -1.44 34.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 34.41) (end 16.68 34.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.68 34.41) (end 16.68 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.68 -1.39) (end -1.44 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -1.6) (end -1.55 34.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 34.65) (end 16.8 34.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.8 34.65) (end 16.8 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.8 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 28 thru_hole oval (at 15.24 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /WR))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /D2))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /A13))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /D1))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /A8))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /D0))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /A9))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /A0))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /A11))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /A1))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /RD))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /A2))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /A10))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /A3))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 /ROMEN))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /A4))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /D7))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 /A5))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /D6))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /A6))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /D5))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 /A7))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /D4))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /A12))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /D3))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /A14))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-28_W15.24mm_Socket_LongPads (layer F.Cu) (tedit 5A02E8C5) (tstamp 605BE9F1)
    (at 20.0279 17.78)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads")
    (path /604FD5C5)
    (fp_text reference U3 (at 7.62 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "256k (32k x 8) SRAM" (at 7.62 35.35) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 16.8 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.8 34.65) (end 16.8 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 34.65) (end 16.8 34.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -1.6) (end -1.55 34.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16.68 -1.39) (end -1.44 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.68 34.41) (end 16.68 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 34.41) (end 16.68 34.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 -1.39) (end -1.44 34.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.68 -1.33) (end 8.62 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 13.68 34.35) (end 13.68 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 34.35) (end 13.68 34.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -1.33) (end 1.56 34.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.62 -1.33) (end 1.56 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 16.51 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 16.51 34.35) (end 16.51 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 34.35) (end 16.51 34.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.33) (end -1.27 34.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0.255 -0.27) (end 1.255 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.255 34.29) (end 0.255 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 14.985 34.29) (end 0.255 34.29) (layer F.Fab) (width 0.1))
    (fp_line (start 14.985 -1.27) (end 14.985 34.29) (layer F.Fab) (width 0.1))
    (fp_line (start 1.255 -1.27) (end 14.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_arc (start 7.62 -1.33) (end 6.62 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 7.62 16.51) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /A14))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /D3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /A12))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /D4))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 /A7))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /D5))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /A6))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /D6))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 /A5))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /D7))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /A4))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /RAMEN))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /A3))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /A10))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /A2))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /RD))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /A1))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /A11))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /A0))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /A9))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /D0))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /A8))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /D1))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /A13))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /D2))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /WR))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 28 thru_hole oval (at 15.24 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-14_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A02E8C5) (tstamp 605BB6C8)
    (at 20.32 63.5)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (path /6051C888)
    (fp_text reference U10 (at 3.81 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 74HC32 (at 3.81 17.57) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 9.15 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.15 16.85) (end 9.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 16.85) (end 9.15 16.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -1.6) (end -1.55 16.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.06 -1.39) (end -1.44 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.06 16.63) (end 9.06 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 16.63) (end 9.06 16.63) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 -1.39) (end -1.44 16.63) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.06 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.06 16.57) (end 6.06 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 16.57) (end 6.06 16.57) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -1.33) (end 1.56 16.57) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.81 -1.33) (end 1.56 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.89 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 16.57) (end 8.89 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 16.57) (end 8.89 16.57) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.33) (end -1.27 16.57) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 16.51) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 16.51) (end 0.635 16.51) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 16.51) (layer F.Fab) (width 0.1))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(U10-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(U10-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /RAMEN))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(U10-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad26)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /A15))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 /ROMEN))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-14_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A02E8C5) (tstamp 605BD47A)
    (at 53.34 63.5)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (path /605236EF)
    (fp_text reference U11 (at 3.81 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 74HC04 (at 3.81 17.57) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 7.62) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 16.51) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 16.51) (end 0.635 16.51) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 16.51) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.33) (end -1.27 16.57) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 16.57) (end 8.89 16.57) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 16.57) (end 8.89 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.56 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -1.33) (end 1.56 16.57) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 16.57) (end 6.06 16.57) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.06 16.57) (end 6.06 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.06 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 -1.39) (end -1.44 16.63) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 16.63) (end 9.06 16.63) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.06 16.63) (end 9.06 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.06 -1.39) (end -1.44 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -1.6) (end -1.55 16.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 16.85) (end 9.15 16.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.15 16.85) (end 9.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.15 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 14 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(U10-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(U11-Pad3)"))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(U10-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /A15))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-16_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A02E8C5) (tstamp 605BB71E)
    (at 119.38 17.78)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (path /60832D85)
    (fp_text reference U20 (at 3.81 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 74HC138 (at 3.81 20.11) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 9.15 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.15 19.4) (end 9.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 19.4) (end 9.15 19.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -1.6) (end -1.55 19.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.06 -1.39) (end -1.44 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.06 19.17) (end 9.06 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 19.17) (end 9.06 19.17) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 -1.39) (end -1.44 19.17) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.06 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.06 19.11) (end 6.06 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 19.11) (end 6.06 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -1.33) (end 1.56 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.81 -1.33) (end 1.56 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.89 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 19.11) (end 8.89 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 19.11) (end 8.89 19.11) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.33) (end -1.27 19.11) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 19.05) (end 0.635 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 /A5))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /IOEN6))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /A6))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /IOEN5))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 /A7))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /IOEN4))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /IORQ))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /IOEN3))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /IORQ))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /IOEN2))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /IOEN1))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /IOEN7))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /IOEN0))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-20_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A02E8C5) (tstamp 605BFB17)
    (at 119.38 43.18)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (path /6057058E)
    (fp_text reference U21 (at 3.81 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 74HC244 (at 3.81 25.19) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 11.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 24.13) (end 0.635 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 24.13) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.33) (end -1.27 24.19) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 24.19) (end 8.89 24.19) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 24.19) (end 8.89 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.56 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -1.33) (end 1.56 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 24.19) (end 6.06 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.06 24.19) (end 6.06 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.06 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 -1.39) (end -1.44 24.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 24.25) (end 9.06 24.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.06 24.25) (end 9.06 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.06 -1.39) (end -1.44 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -1.6) (end -1.55 24.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 24.45) (end 9.15 24.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.15 24.45) (end 9.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.15 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 20 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /IORQ))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /IOWR))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(U21-Pad18)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /A3))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /A0))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /IOADDR0))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(U21-Pad16)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /A4))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /A1))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /IOADDR1))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /IOADDR4))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(U21-Pad4)"))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /A2))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /IOADDR2))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /IOADDR3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(U21-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /WR))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /IORQ))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-20_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A02E8C5) (tstamp 605BB77E)
    (at 119.38 73.66)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (path /608489B5)
    (fp_text reference U22 (at 3.81 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 74HC245 (at 3.81 25.19) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 9.15 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.15 24.45) (end 9.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 24.45) (end 9.15 24.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -1.6) (end -1.55 24.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.06 -1.39) (end -1.44 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.06 24.25) (end 9.06 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 24.25) (end 9.06 24.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.44 -1.39) (end -1.44 24.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.06 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.06 24.19) (end 6.06 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 24.19) (end 6.06 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -1.33) (end 1.56 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.81 -1.33) (end 1.56 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.89 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 24.19) (end 8.89 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 24.19) (end 8.89 24.19) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.33) (end -1.27 24.19) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 24.13) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 24.13) (end 0.635 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /WR))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /D7))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /IOD0))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /D6))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /IOD1))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /D5))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /IOD2))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /D4))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /IOD3))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /D3))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /IOD4))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /D2))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /IOD5))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /D1))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /IOD6))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /D0))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /IOD7))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /IORQ))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D) (tstamp 605BB798)
    (at 98.939001 198.719001)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (path /60B8B756)
    (fp_text reference U30 (at 2.54 -4.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM7805_TO220 (at 2.54 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.79 -3.4) (end -2.71 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.79 1.51) (end 7.79 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.71 1.51) (end 7.79 1.51) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.71 -3.4) (end -2.71 1.51) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.391 -3.27) (end 4.391 -1.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.69 -3.27) (end 0.69 -1.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 -1.76) (end 7.66 -1.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 -3.27) (end 7.66 1.371) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 -3.27) (end -2.58 1.371) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 1.371) (end 7.66 1.371) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 -3.27) (end 7.66 -3.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.39 -3.15) (end 4.39 -1.88) (layer F.Fab) (width 0.1))
    (fp_line (start 0.69 -3.15) (end 0.69 -1.88) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 -1.88) (end 7.54 -1.88) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 -3.15) (end -2.46 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 1.25) (end 7.54 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 1.25) (end 7.54 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 -3.15) (end -2.46 1.25) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.54 -4.27) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Crystal:Crystal_HC18-U_Vertical (layer F.Cu) (tedit 5A1AD3B7) (tstamp 605BB7AF)
    (at 54.61 85.09)
    (descr "Crystal THT HC-18/U, http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-18/U")
    (path /6058BCE7)
    (fp_text reference Y1 (at 2.45 -3.525) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4Mhz (at 2.45 3.525) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.4 -2.8) (end -3.5 -2.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.4 2.8) (end 8.4 -2.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.5 2.8) (end 8.4 2.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.5 -2.8) (end -3.5 2.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.675 2.525) (end 5.575 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.675 -2.525) (end 5.575 -2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.55 2) (end 5.45 2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.55 -2) (end 5.45 -2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.675 2.325) (end 5.575 2.325) (layer F.Fab) (width 0.1))
    (fp_line (start -0.675 -2.325) (end 5.575 -2.325) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 2.45 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start -0.675 0) (end -0.675 -2.325) (angle -180) (layer F.Fab) (width 0.1))
    (fp_arc (start 5.575 0) (end 5.575 -2.325) (angle 180) (layer F.Fab) (width 0.1))
    (fp_arc (start -0.55 0) (end -0.55 -2) (angle -180) (layer F.Fab) (width 0.1))
    (fp_arc (start 5.45 0) (end 5.45 -2) (angle 180) (layer F.Fab) (width 0.1))
    (fp_arc (start -0.675 0) (end -0.675 -2.525) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_arc (start 5.575 0) (end 5.575 -2.525) (angle 180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 4.9 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC18-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (segment (start 27.94 73.66) (end 53.34 73.66) (width 0.25) (layer B.Cu) (net 0))
  (segment (start 53.34 73.66) (end 53.34 78.74) (width 0.25) (layer B.Cu) (net 0))
  (segment (start 27.94 78.74) (end 20.32 78.74) (width 0.25) (layer B.Cu) (net 0))
  (segment (start 27.94 63.5) (end 48.26 63.5) (width 0.25) (layer B.Cu) (net 0))
  (segment (start 48.26 63.5) (end 50.8 60.96) (width 0.25) (layer B.Cu) (net 0))
  (segment (start 58.42 60.96) (end 60.96 63.5) (width 0.25) (layer B.Cu) (net 0))
  (segment (start 50.8 60.96) (end 58.42 60.96) (width 0.25) (layer B.Cu) (net 0))
  (segment (start 21.15291 51.92501) (end 43.32499 51.92501) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 20.0279 50.8) (end 21.15291 51.92501) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 44.45 50.8) (end 53.34 50.8) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 43.32499 51.92501) (end 44.45 50.8) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 99.06 45.72) (end 101.6 45.72) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 90.17 54.61) (end 99.06 45.72) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 63.5 54.61) (end 90.17 54.61) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 53.34 50.8) (end 59.69 50.8) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 59.69 50.8) (end 63.5 54.61) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 53.34 100.25) (end 60.96 100.25) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 60.96 66.04) (end 58.42 66.04) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 58.42 66.04) (end 55.88 68.58) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 55.88 83.82) (end 54.61 85.09) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 55.88 68.58) (end 55.88 83.82) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 54.61 90.17) (end 53.34 91.44) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 54.61 85.09) (end 54.61 90.17) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 53.34 91.44) (end 53.34 95.25) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 59.51 85.09) (end 59.69 85.09) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 60.96 68.58) (end 60.96 71.12) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 58.42 84) (end 59.51 85.09) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 60.96 68.58) (end 58.42 68.58) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 58.42 68.58) (end 58.42 84) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 59.51 89.99) (end 60.96 91.44) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 59.51 85.09) (end 59.51 89.99) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 60.96 91.44) (end 60.96 95.25) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 36.392901 16.654999) (end 59.834999 16.654999) (width 0.5) (layer B.Cu) (net 6))
  (segment (start 35.2679 17.78) (end 36.392901 16.654999) (width 0.5) (layer B.Cu) (net 6))
  (segment (start 60.96 17.78) (end 68.58 17.78) (width 0.5) (layer B.Cu) (net 6))
  (segment (start 59.834999 16.654999) (end 60.96 17.78) (width 0.5) (layer B.Cu) (net 6))
  (segment (start 127 20.32) (end 144.78 20.32) (width 0.25) (layer B.Cu) (net 10))
  (segment (start 144.78 20.32) (end 160.02 20.32) (width 0.25) (layer B.Cu) (net 10))
  (segment (start 127 22.86) (end 144.78 22.86) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 144.78 22.86) (end 160.02 22.86) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 127 25.4) (end 144.78 25.4) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 144.78 25.4) (end 160.02 25.4) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 127 27.94) (end 144.78 27.94) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 144.78 27.94) (end 160.02 27.94) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 127 30.48) (end 144.78 30.48) (width 0.25) (layer B.Cu) (net 14))
  (segment (start 144.78 30.48) (end 160.02 30.48) (width 0.25) (layer B.Cu) (net 14))
  (segment (start 127 33.02) (end 144.78 33.02) (width 0.25) (layer B.Cu) (net 15))
  (segment (start 144.78 33.02) (end 160.02 33.02) (width 0.25) (layer B.Cu) (net 15))
  (segment (start 127 35.56) (end 144.78 35.56) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 144.78 35.56) (end 160.02 35.56) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 160.02 38.1) (end 144.78 38.1) (width 0.25) (layer B.Cu) (net 17))
  (segment (start 144.78 38.1) (end 125.73 38.1) (width 0.25) (layer B.Cu) (net 17))
  (segment (start 125.73 38.1) (end 120.65 33.02) (width 0.25) (layer B.Cu) (net 17))
  (segment (start 120.65 33.02) (end 119.38 33.02) (width 0.25) (layer B.Cu) (net 17))
  (segment (start 160.02 40.64) (end 161.29 40.64) (width 0.25) (layer B.Cu) (net 18) (tstamp 605C0505))
  (segment (start 161.29 40.64) (end 162.56 41.91) (width 0.25) (layer B.Cu) (net 18) (tstamp 605C00B2))
  (segment (start 162.56 41.91) (end 162.56 43.18) (width 0.25) (layer B.Cu) (net 18) (tstamp 605C0502))
  (segment (start 162.56 43.18) (end 161.29 44.45) (width 0.25) (layer B.Cu) (net 18) (tstamp 605C00B5))
  (segment (start 161.29 44.45) (end 144.78 44.45) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 132.08 57.15) (end 124.46 57.15) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 124.46 57.15) (end 123.19 58.42) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 123.19 58.42) (end 119.38 58.42) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 132.08 57.15) (end 144.78 44.45) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 160.02 43.18) (end 144.78 43.18) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 133.35 54.61) (end 124.46 54.61) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 123.19 53.34) (end 119.38 53.34) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 124.46 54.61) (end 123.19 53.34) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 133.35 54.61) (end 144.78 43.18) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 161.222081 45.72) (end 163.83 43.112081) (width 0.25) (layer B.Cu) (net 20) (tstamp 605C050B))
  (segment (start 160.02 45.72) (end 161.222081 45.72) (width 0.25) (layer B.Cu) (net 20) (tstamp 605C00B8))
  (segment (start 163.83 43.112081) (end 163.83 41.91) (width 0.25) (layer B.Cu) (net 20) (tstamp 605C0508))
  (segment (start 163.83 41.91) (end 161.29 39.37) (width 0.25) (layer B.Cu) (net 20) (tstamp 605C00AC))
  (segment (start 161.29 39.37) (end 146.05 39.37) (width 0.25) (layer B.Cu) (net 20))
  (segment (start 135.89 49.53) (end 123.19 49.53) (width 0.25) (layer B.Cu) (net 20))
  (segment (start 121.92 48.26) (end 119.38 48.26) (width 0.25) (layer B.Cu) (net 20))
  (segment (start 123.19 49.53) (end 121.92 48.26) (width 0.25) (layer B.Cu) (net 20))
  (segment (start 135.89 49.53) (end 146.05 39.37) (width 0.25) (layer B.Cu) (net 20))
  (segment (start 127 63.5) (end 142.24 63.5) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 153.764999 51.975001) (end 161.384999 51.975001) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 162.56 50.8) (end 162.56 49.53) (width 0.25) (layer B.Cu) (net 21) (tstamp 605C04FF))
  (segment (start 161.29 48.26) (end 160.02 48.26) (width 0.25) (layer B.Cu) (net 21) (tstamp 605C04FC))
  (segment (start 161.384999 51.975001) (end 162.56 50.8) (width 0.25) (layer B.Cu) (net 21) (tstamp 605C04F9))
  (segment (start 162.56 49.53) (end 161.29 48.26) (width 0.25) (layer B.Cu) (net 21) (tstamp 605C00AF))
  (segment (start 153.764999 51.975001) (end 142.24 63.5) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 160.02 50.8) (end 153.67 50.8) (width 0.25) (layer B.Cu) (net 22))
  (segment (start 146.05 58.42) (end 127 58.42) (width 0.25) (layer B.Cu) (net 22))
  (segment (start 146.05 58.42) (end 153.67 50.8) (width 0.25) (layer B.Cu) (net 22))
  (segment (start 160.02 53.34) (end 153.67 53.34) (width 0.25) (layer B.Cu) (net 23))
  (segment (start 131.93501 75.07499) (end 123.04501 75.07499) (width 0.25) (layer B.Cu) (net 23))
  (segment (start 121.92 76.2) (end 119.38 76.2) (width 0.25) (layer B.Cu) (net 23))
  (segment (start 123.04501 75.07499) (end 121.92 76.2) (width 0.25) (layer B.Cu) (net 23))
  (segment (start 153.67 53.34) (end 131.93501 75.07499) (width 0.25) (layer B.Cu) (net 23))
  (segment (start 160.02 55.88) (end 153.67 55.88) (width 0.25) (layer B.Cu) (net 24))
  (segment (start 131.93501 77.61499) (end 123.04501 77.61499) (width 0.25) (layer B.Cu) (net 24))
  (segment (start 121.92 78.74) (end 119.38 78.74) (width 0.25) (layer B.Cu) (net 24))
  (segment (start 123.04501 77.61499) (end 121.92 78.74) (width 0.25) (layer B.Cu) (net 24))
  (segment (start 131.93501 77.61499) (end 153.67 55.88) (width 0.25) (layer B.Cu) (net 24))
  (segment (start 160.02 58.42) (end 153.67 58.42) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 131.93501 80.15499) (end 123.04501 80.15499) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 121.92 81.28) (end 119.38 81.28) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 123.04501 80.15499) (end 121.92 81.28) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 153.67 58.42) (end 131.93501 80.15499) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 160.02 60.96) (end 153.67 60.96) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 132.08 82.55) (end 123.19 82.55) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 121.92 83.82) (end 119.38 83.82) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 123.19 82.55) (end 121.92 83.82) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 153.67 60.96) (end 132.08 82.55) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 160.02 63.5) (end 153.67 63.5) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 132.08 85.09) (end 123.19 85.09) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 121.92 86.36) (end 119.38 86.36) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 123.19 85.09) (end 121.92 86.36) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 153.67 63.5) (end 132.08 85.09) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 160.02 66.04) (end 153.67 66.04) (width 0.25) (layer B.Cu) (net 28))
  (segment (start 132.08 87.63) (end 123.19 87.63) (width 0.25) (layer B.Cu) (net 28))
  (segment (start 121.92 88.9) (end 119.38 88.9) (width 0.25) (layer B.Cu) (net 28))
  (segment (start 123.19 87.63) (end 121.92 88.9) (width 0.25) (layer B.Cu) (net 28))
  (segment (start 153.67 66.04) (end 132.08 87.63) (width 0.25) (layer B.Cu) (net 28))
  (segment (start 160.02 68.58) (end 153.67 68.58) (width 0.25) (layer B.Cu) (net 29))
  (segment (start 131.93501 90.31499) (end 123.33499 90.31499) (width 0.25) (layer B.Cu) (net 29))
  (segment (start 122.20998 91.44) (end 119.38 91.44) (width 0.25) (layer B.Cu) (net 29))
  (segment (start 123.33499 90.31499) (end 122.20998 91.44) (width 0.25) (layer B.Cu) (net 29))
  (segment (start 153.67 68.58) (end 131.93501 90.31499) (width 0.25) (layer B.Cu) (net 29))
  (segment (start 160.02 71.12) (end 153.67 71.12) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 132.08 92.71) (end 123.19 92.71) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 121.92 93.98) (end 119.38 93.98) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 123.19 92.71) (end 121.92 93.98) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 132.08 92.71) (end 153.67 71.12) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 160.02 73.66) (end 153.67 73.66) (width 0.25) (layer B.Cu) (net 31))
  (via (at 153.67 73.66) (size 1.5) (drill 0.5) (layers F.Cu B.Cu) (net 31))
  (segment (start 132.08 64.77) (end 123.19 64.77) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 121.92 63.5) (end 119.38 63.5) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 123.19 64.77) (end 121.92 63.5) (width 0.25) (layer B.Cu) (net 31))
  (via (at 131.95486 73.53486) (size 1.5) (drill 0.5) (layers F.Cu B.Cu) (net 31))
  (segment (start 132.08 64.77) (end 132.08 73.40972) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 132.08 73.40972) (end 131.95486 73.53486) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 153.54486 73.53486) (end 153.67 73.66) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 131.95486 73.53486) (end 153.54486 73.53486) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 35.2679 30.48) (end 43.18 30.48) (width 0.25) (layer B.Cu) (net 34))
  (segment (start 43.18 30.48) (end 44.45 29.21) (width 0.25) (layer B.Cu) (net 34))
  (segment (start 44.45 29.21) (end 59.69 29.21) (width 0.25) (layer B.Cu) (net 34))
  (segment (start 60.96 30.48) (end 68.58 30.48) (width 0.25) (layer B.Cu) (net 34))
  (segment (start 59.69 29.21) (end 60.96 30.48) (width 0.25) (layer B.Cu) (net 34))
  (segment (start 35.2679 33.02) (end 43.18 33.02) (width 0.25) (layer B.Cu) (net 35))
  (segment (start 43.18 33.02) (end 44.45 31.75) (width 0.25) (layer B.Cu) (net 35))
  (segment (start 44.45 31.75) (end 59.69 31.75) (width 0.25) (layer B.Cu) (net 35))
  (segment (start 60.96 33.02) (end 68.58 33.02) (width 0.25) (layer B.Cu) (net 35))
  (segment (start 59.69 31.75) (end 60.96 33.02) (width 0.25) (layer B.Cu) (net 35))
  (segment (start 21.15291 21.44501) (end 43.32499 21.44501) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 20.0279 20.32) (end 21.15291 21.44501) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 44.45 20.32) (end 53.34 20.32) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 43.32499 21.44501) (end 44.45 20.32) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 53.34 20.32) (end 59.69 20.32) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 59.69 20.32) (end 60.96 21.59) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 60.96 21.59) (end 78.74 21.59) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 78.74 21.59) (end 80.01 20.32) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 80.01 20.32) (end 86.36 20.32) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 35.71791 19.86999) (end 43.63001 19.86999) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 35.2679 20.32) (end 35.71791 19.86999) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 44.30501 19.19499) (end 59.83499 19.19499) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 43.63001 19.86999) (end 44.30501 19.19499) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 60.96 20.32) (end 68.58 20.32) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 59.83499 19.19499) (end 60.96 20.32) (width 0.25) (layer B.Cu) (net 37))
  (via (at 77.47 20.32) (size 1.5) (drill 0.5) (layers F.Cu B.Cu) (net 37))
  (segment (start 68.58 20.32) (end 77.47 20.32) (width 0.25) (layer B.Cu) (net 37))
  (via (at 77.47 64.77) (size 1.5) (drill 0.5) (layers F.Cu B.Cu) (net 37))
  (segment (start 77.47 20.32) (end 77.47 64.77) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 77.47 64.77) (end 92.71 64.77) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 93.98 63.5) (end 101.6 63.5) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 92.71 64.77) (end 93.98 63.5) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 127 66.04) (end 119.38 73.66) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 60.96 22.86) (end 68.58 22.86) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 59.83499 21.73499) (end 60.96 22.86) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 35.2679 22.86) (end 43.81359 22.86) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 44.9386 21.73499) (end 59.83499 21.73499) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 43.81359 22.86) (end 44.9386 21.73499) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 86.36 22.86) (end 68.58 22.86) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 21.44289 19.19499) (end 43.03501 19.19499) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 20.0279 17.78) (end 21.44289 19.19499) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 44.45 17.78) (end 53.34 17.78) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 43.03501 19.19499) (end 44.45 17.78) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 53.34 17.78) (end 59.69 17.78) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 59.69 17.78) (end 60.96 19.05) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 60.96 19.05) (end 82.55 19.05) (width 0.25) (layer B.Cu) (net 40))
  (via (at 82.55 19.05) (size 1.5) (drill 0.5) (layers F.Cu B.Cu) (net 40))
  (via (at 82.55 25.4) (size 1.5) (drill 0.5) (layers F.Cu B.Cu) (net 40))
  (segment (start 82.55 19.05) (end 82.55 25.4) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 82.55 25.4) (end 86.36 25.4) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 101.6 53.34) (end 93.98 53.34) (width 0.25) (layer B.Cu) (net 43))
  (segment (start 53.916014 67.45499) (end 46.84501 67.45499) (width 0.25) (layer B.Cu) (net 43))
  (segment (start 61.536014 64.91499) (end 56.456014 64.91499) (width 0.25) (layer B.Cu) (net 43))
  (segment (start 56.456014 64.91499) (end 53.916014 67.45499) (width 0.25) (layer B.Cu) (net 43))
  (segment (start 69.445994 57.00501) (end 61.536014 64.91499) (width 0.25) (layer B.Cu) (net 43))
  (segment (start 93.98 53.34) (end 90.31499 57.00501) (width 0.25) (layer B.Cu) (net 43))
  (segment (start 90.31499 57.00501) (end 69.445994 57.00501) (width 0.25) (layer B.Cu) (net 43))
  (segment (start 43.18 71.12) (end 27.94 71.12) (width 0.25) (layer B.Cu) (net 43))
  (segment (start 46.84501 67.45499) (end 43.18 71.12) (width 0.25) (layer B.Cu) (net 43))
  (segment (start 35.2679 48.26) (end 43.18 48.26) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 43.18 48.26) (end 44.45 46.99) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 44.45 46.99) (end 59.69 46.99) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 59.69 46.99) (end 60.96 48.26) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 60.96 48.26) (end 68.58 48.26) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 35.2679 50.8) (end 43.18 50.8) (width 0.25) (layer B.Cu) (net 46))
  (segment (start 43.18 50.8) (end 44.45 49.53) (width 0.25) (layer B.Cu) (net 46))
  (segment (start 44.45 49.53) (end 59.69 49.53) (width 0.25) (layer B.Cu) (net 46))
  (segment (start 59.69 49.53) (end 60.96 50.8) (width 0.25) (layer B.Cu) (net 46))
  (segment (start 60.96 50.8) (end 68.58 50.8) (width 0.25) (layer B.Cu) (net 46))
  (segment (start 35.2679 45.72) (end 43.18 45.72) (width 0.25) (layer B.Cu) (net 48))
  (segment (start 43.18 45.72) (end 44.45 44.45) (width 0.25) (layer B.Cu) (net 48))
  (segment (start 44.45 44.45) (end 59.69 44.45) (width 0.25) (layer B.Cu) (net 48))
  (segment (start 59.69 44.45) (end 60.96 45.72) (width 0.25) (layer B.Cu) (net 48))
  (segment (start 60.96 45.72) (end 68.58 45.72) (width 0.25) (layer B.Cu) (net 48))
  (segment (start 35.2679 43.18) (end 43.18 43.18) (width 0.25) (layer B.Cu) (net 49))
  (segment (start 43.18 43.18) (end 44.45 41.91) (width 0.25) (layer B.Cu) (net 49))
  (segment (start 44.45 41.91) (end 59.69 41.91) (width 0.25) (layer B.Cu) (net 49))
  (segment (start 59.69 41.91) (end 60.96 43.18) (width 0.25) (layer B.Cu) (net 49))
  (segment (start 60.96 43.18) (end 68.58 43.18) (width 0.25) (layer B.Cu) (net 49))
  (segment (start 21.15291 41.76501) (end 43.32499 41.76501) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 20.0279 40.64) (end 21.15291 41.76501) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 44.45 40.64) (end 53.34 40.64) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 43.32499 41.76501) (end 44.45 40.64) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 53.34 40.64) (end 59.69 40.64) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 59.69 40.64) (end 60.96 41.91) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 60.96 41.91) (end 92.71 41.91) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 92.71 41.91) (end 93.98 43.18) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 93.98 43.18) (end 101.6 43.18) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 21.15291 39.22501) (end 43.32499 39.22501) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 20.0279 38.1) (end 21.15291 39.22501) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 44.45 38.1) (end 53.34 38.1) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 43.32499 39.22501) (end 44.45 38.1) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 53.34 38.1) (end 59.69 38.1) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 59.69 38.1) (end 60.96 39.37) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 60.96 39.37) (end 92.71 39.37) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 92.71 39.37) (end 93.98 40.64) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 93.98 40.64) (end 101.6 40.64) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 21.15291 49.38501) (end 43.32499 49.38501) (width 0.25) (layer B.Cu) (net 52))
  (segment (start 20.0279 48.26) (end 21.15291 49.38501) (width 0.25) (layer B.Cu) (net 52))
  (segment (start 44.45 48.26) (end 53.34 48.26) (width 0.25) (layer B.Cu) (net 52))
  (segment (start 43.32499 49.38501) (end 44.45 48.26) (width 0.25) (layer B.Cu) (net 52))
  (segment (start 53.34 48.26) (end 60.32359 48.26) (width 0.25) (layer B.Cu) (net 52))
  (via (at 76.2 49.53) (size 1.5) (drill 0.5) (layers F.Cu B.Cu) (net 52))
  (segment (start 61.59359 49.53) (end 76.2 49.53) (width 0.25) (layer B.Cu) (net 52))
  (segment (start 60.32359 48.26) (end 61.59359 49.53) (width 0.25) (layer B.Cu) (net 52))
  (segment (start 76.2 49.53) (end 76.2 43.18) (width 0.25) (layer F.Cu) (net 52))
  (via (at 76.2 43.18) (size 1.5) (drill 0.5) (layers F.Cu B.Cu) (net 52))
  (segment (start 76.2 43.18) (end 80.01 43.18) (width 0.25) (layer B.Cu) (net 52))
  (segment (start 82.55 45.72) (end 86.36 45.72) (width 0.25) (layer B.Cu) (net 52))
  (segment (start 80.01 43.18) (end 82.55 45.72) (width 0.25) (layer B.Cu) (net 52))
  (segment (start 44.45 35.56) (end 53.34 35.56) (width 0.25) (layer B.Cu) (net 53))
  (segment (start 43.32499 36.68501) (end 44.45 35.56) (width 0.25) (layer B.Cu) (net 53))
  (segment (start 43.32499 36.68501) (end 28.08499 36.68501) (width 0.25) (layer B.Cu) (net 53))
  (segment (start 28.08499 36.68501) (end 26.95998 35.56) (width 0.25) (layer B.Cu) (net 53))
  (segment (start 26.95998 35.56) (end 20.0279 35.56) (width 0.25) (layer B.Cu) (net 53))
  (segment (start 53.34 35.56) (end 59.69 35.56) (width 0.25) (layer B.Cu) (net 53))
  (segment (start 59.69 35.56) (end 60.96 36.83) (width 0.25) (layer B.Cu) (net 53))
  (segment (start 60.96 36.83) (end 92.71 36.83) (width 0.25) (layer B.Cu) (net 53))
  (segment (start 92.71 36.83) (end 93.98 38.1) (width 0.25) (layer B.Cu) (net 53))
  (segment (start 93.98 38.1) (end 101.6 38.1) (width 0.25) (layer B.Cu) (net 53))
  (segment (start 35.2679 40.64) (end 43.18 40.64) (width 0.25) (layer B.Cu) (net 54))
  (segment (start 43.18 40.64) (end 44.45 39.37) (width 0.25) (layer B.Cu) (net 54))
  (segment (start 44.45 39.37) (end 59.69 39.37) (width 0.25) (layer B.Cu) (net 54))
  (segment (start 59.69 39.37) (end 60.96 40.64) (width 0.25) (layer B.Cu) (net 54))
  (segment (start 60.96 40.64) (end 68.58 40.64) (width 0.25) (layer B.Cu) (net 54))
  (segment (start 21.15291 34.14501) (end 43.32499 34.14501) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 20.0279 33.02) (end 21.15291 34.14501) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 44.45 33.02) (end 53.34 33.02) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 43.32499 34.14501) (end 44.45 33.02) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 53.34 33.02) (end 59.69 33.02) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 59.69 33.02) (end 60.96 34.29) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 60.96 34.29) (end 92.71 34.29) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 92.71 34.29) (end 93.98 35.56) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 93.98 35.56) (end 101.6 35.56) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 101.6 35.56) (end 110.49 44.45) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 110.49 44.45) (end 110.49 52.07) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 110.49 52.07) (end 119.38 60.96) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 21.15291 44.30501) (end 43.32499 44.30501) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 20.0279 43.18) (end 21.15291 44.30501) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 44.45 43.18) (end 53.34 43.18) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 43.32499 44.30501) (end 44.45 43.18) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 53.34 43.18) (end 59.69 43.18) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 59.69 43.18) (end 60.96 44.45) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 60.96 44.45) (end 76.2 44.45) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 76.2 44.45) (end 82.55 50.8) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 82.55 50.8) (end 86.36 50.8) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 92.71 44.45) (end 86.36 50.8) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 109.22 44.45) (end 92.71 44.45) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 121.92 80.01) (end 115.57 80.01) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 123.19 78.74) (end 121.92 80.01) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 115.57 58.42) (end 109.22 52.07) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 127 78.74) (end 123.19 78.74) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 115.57 80.01) (end 115.57 58.42) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 109.22 52.07) (end 109.22 44.45) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 21.15291 31.60501) (end 43.32499 31.60501) (width 0.25) (layer B.Cu) (net 57))
  (segment (start 20.0279 30.48) (end 21.15291 31.60501) (width 0.25) (layer B.Cu) (net 57))
  (segment (start 44.45 30.48) (end 53.34 30.48) (width 0.25) (layer B.Cu) (net 57))
  (segment (start 43.32499 31.60501) (end 44.45 30.48) (width 0.25) (layer B.Cu) (net 57))
  (segment (start 53.34 30.48) (end 59.69 30.48) (width 0.25) (layer B.Cu) (net 57))
  (segment (start 59.69 30.48) (end 60.96 31.75) (width 0.25) (layer B.Cu) (net 57))
  (segment (start 60.96 31.75) (end 92.71 31.75) (width 0.25) (layer B.Cu) (net 57))
  (segment (start 92.71 31.75) (end 93.98 33.02) (width 0.25) (layer B.Cu) (net 57))
  (segment (start 93.98 33.02) (end 101.6 33.02) (width 0.25) (layer B.Cu) (net 57))
  (segment (start 101.6 33.02) (end 111.76 43.18) (width 0.25) (layer B.Cu) (net 57))
  (segment (start 111.76 48.26) (end 119.38 55.88) (width 0.25) (layer B.Cu) (net 57))
  (segment (start 111.76 43.18) (end 111.76 48.26) (width 0.25) (layer B.Cu) (net 57))
  (segment (start 21.15291 46.84501) (end 43.32499 46.84501) (width 0.25) (layer B.Cu) (net 58))
  (segment (start 20.0279 45.72) (end 21.15291 46.84501) (width 0.25) (layer B.Cu) (net 58))
  (segment (start 44.45 45.72) (end 53.34 45.72) (width 0.25) (layer B.Cu) (net 58))
  (segment (start 43.32499 46.84501) (end 44.45 45.72) (width 0.25) (layer B.Cu) (net 58))
  (segment (start 53.34 45.72) (end 59.69 45.72) (width 0.25) (layer B.Cu) (net 58))
  (segment (start 59.69 45.72) (end 60.96 46.99) (width 0.25) (layer B.Cu) (net 58))
  (segment (start 60.96 46.99) (end 76.2 46.99) (width 0.25) (layer B.Cu) (net 58))
  (segment (start 76.2 46.99) (end 82.55 53.34) (width 0.25) (layer B.Cu) (net 58))
  (segment (start 82.55 53.34) (end 86.36 53.34) (width 0.25) (layer B.Cu) (net 58))
  (segment (start 21.15291 29.06501) (end 43.32499 29.06501) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 20.0279 27.94) (end 21.15291 29.06501) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 44.45 27.94) (end 53.34 27.94) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 43.32499 29.06501) (end 44.45 27.94) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 53.34 27.94) (end 59.69 27.94) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 59.69 27.94) (end 60.96 29.21) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 60.96 29.21) (end 92.71 29.21) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 92.71 29.21) (end 93.98 30.48) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 93.98 30.48) (end 101.6 30.48) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 121.92 17.78) (end 119.38 17.78) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 120.79499 21.44501) (end 121.92 20.32) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 121.92 20.32) (end 121.92 17.78) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 114.44499 21.44501) (end 120.79499 21.44501) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 101.6 30.48) (end 105.41 30.48) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 105.41 30.48) (end 114.44499 21.44501) (width 0.25) (layer B.Cu) (net 59))
  (segment (start 21.15291 26.52501) (end 43.32499 26.52501) (width 0.25) (layer B.Cu) (net 60))
  (segment (start 20.0279 25.4) (end 21.15291 26.52501) (width 0.25) (layer B.Cu) (net 60))
  (segment (start 44.45 25.4) (end 53.34 25.4) (width 0.25) (layer B.Cu) (net 60))
  (segment (start 43.32499 26.52501) (end 44.45 25.4) (width 0.25) (layer B.Cu) (net 60))
  (segment (start 53.34 25.4) (end 59.69 25.4) (width 0.25) (layer B.Cu) (net 60))
  (segment (start 59.69 25.4) (end 60.96 26.67) (width 0.25) (layer B.Cu) (net 60))
  (segment (start 60.96 26.67) (end 92.71 26.67) (width 0.25) (layer B.Cu) (net 60))
  (segment (start 92.71 26.67) (end 93.98 27.94) (width 0.25) (layer B.Cu) (net 60))
  (segment (start 93.98 27.94) (end 101.6 27.94) (width 0.25) (layer B.Cu) (net 60))
  (segment (start 101.6 27.94) (end 105.41 27.94) (width 0.25) (layer B.Cu) (net 60))
  (segment (start 105.41 27.94) (end 113.03 20.32) (width 0.25) (layer B.Cu) (net 60))
  (segment (start 113.03 20.32) (end 119.38 20.32) (width 0.25) (layer B.Cu) (net 60))
  (segment (start 21.15291 23.98501) (end 43.32499 23.98501) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 20.0279 22.86) (end 21.15291 23.98501) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 44.45 22.86) (end 53.34 22.86) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 43.32499 23.98501) (end 44.45 22.86) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 92.71 24.13) (end 93.98 25.4) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 60.96 24.13) (end 92.71 24.13) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 53.34 22.86) (end 59.69 22.86) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 93.98 25.4) (end 101.6 25.4) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 59.69 22.86) (end 60.96 24.13) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 101.6 25.4) (end 105.41 25.4) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 105.41 25.4) (end 115.57 15.24) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 115.57 15.24) (end 121.92 15.24) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 121.92 15.24) (end 123.19 16.51) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 120.83 22.86) (end 119.38 22.86) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 123.19 20.5) (end 120.83 22.86) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 123.19 16.51) (end 123.19 20.5) (width 0.25) (layer B.Cu) (net 61))
  (segment (start 35.2679 25.4) (end 43.18 25.4) (width 0.25) (layer B.Cu) (net 62))
  (segment (start 43.18 25.4) (end 44.45 24.13) (width 0.25) (layer B.Cu) (net 62))
  (segment (start 44.45 24.13) (end 59.69 24.13) (width 0.25) (layer B.Cu) (net 62))
  (segment (start 60.96 25.4) (end 68.58 25.4) (width 0.25) (layer B.Cu) (net 62))
  (segment (start 59.69 24.13) (end 60.96 25.4) (width 0.25) (layer B.Cu) (net 62))
  (segment (start 35.2679 27.94) (end 43.18 27.94) (width 0.25) (layer B.Cu) (net 64))
  (segment (start 43.18 27.94) (end 44.45 26.67) (width 0.25) (layer B.Cu) (net 64))
  (segment (start 44.45 26.67) (end 59.69 26.67) (width 0.25) (layer B.Cu) (net 64))
  (segment (start 60.96 27.94) (end 68.58 27.94) (width 0.25) (layer B.Cu) (net 64))
  (segment (start 59.69 26.67) (end 60.96 27.94) (width 0.25) (layer B.Cu) (net 64))
  (segment (start 127 76.2) (end 130.81 76.2) (width 0.25) (layer B.Cu) (net 65))
  (via (at 130.81 76.2) (size 1.5) (drill 0.5) (layers F.Cu B.Cu) (net 65))
  (segment (start 130.81 76.2) (end 130.81 40.64) (width 0.25) (layer F.Cu) (net 65))
  (via (at 130.81 40.64) (size 1.5) (drill 0.5) (layers F.Cu B.Cu) (net 65))
  (segment (start 121.92 40.64) (end 119.38 43.18) (width 0.25) (layer B.Cu) (net 65))
  (segment (start 130.81 40.64) (end 121.92 40.64) (width 0.25) (layer B.Cu) (net 65))
  (segment (start 119.38 43.18) (end 121.92 43.18) (width 0.25) (layer B.Cu) (net 65))
  (segment (start 124.46 45.72) (end 127 45.72) (width 0.25) (layer B.Cu) (net 65))
  (segment (start 121.92 43.18) (end 124.46 45.72) (width 0.25) (layer B.Cu) (net 65))
  (segment (start 119.38 43.18) (end 116.84 40.64) (width 0.25) (layer B.Cu) (net 65))
  (segment (start 118.11 27.94) (end 119.38 27.94) (width 0.25) (layer B.Cu) (net 65))
  (segment (start 116.84 29.21) (end 118.11 27.94) (width 0.25) (layer B.Cu) (net 65))
  (segment (start 116.84 40.64) (end 116.84 29.21) (width 0.25) (layer B.Cu) (net 65))
  (segment (start 116.84 29.21) (end 116.84 26.67) (width 0.25) (layer B.Cu) (net 65))
  (segment (start 116.84 26.67) (end 118.11 25.4) (width 0.25) (layer B.Cu) (net 65))
  (segment (start 118.11 25.4) (end 119.38 25.4) (width 0.25) (layer B.Cu) (net 65))
  (segment (start 35.2679 35.56) (end 43.18 35.56) (width 0.25) (layer B.Cu) (net 66))
  (segment (start 43.18 35.56) (end 44.45 34.29) (width 0.25) (layer B.Cu) (net 66))
  (segment (start 44.45 34.29) (end 59.69 34.29) (width 0.25) (layer B.Cu) (net 66))
  (segment (start 59.69 34.29) (end 60.96 35.56) (width 0.25) (layer B.Cu) (net 66))
  (segment (start 60.96 35.56) (end 68.58 35.56) (width 0.25) (layer B.Cu) (net 66))
  (segment (start 68.58 38.1) (end 60.96 38.1) (width 0.25) (layer B.Cu) (net 67))
  (segment (start 60.96 38.1) (end 59.69 36.83) (width 0.25) (layer B.Cu) (net 67))
  (segment (start 59.69 36.83) (end 44.45 36.83) (width 0.25) (layer B.Cu) (net 67))
  (segment (start 44.45 36.83) (end 43.18 38.1) (width 0.25) (layer B.Cu) (net 67))
  (segment (start 43.18 38.1) (end 40.64 38.1) (width 0.25) (layer B.Cu) (net 67))
  (segment (start 40.64 38.1) (end 40.64 38.1) (width 0.25) (layer B.Cu) (net 67) (tstamp 605BF917))
  (via (at 40.64 38.1) (size 1.5) (drill 0.5) (layers F.Cu B.Cu) (net 67))
  (segment (start 40.64 38.1) (end 40.64 57.15) (width 0.25) (layer F.Cu) (net 67))
  (via (at 40.64 77.47) (size 1.5) (drill 0.5) (layers F.Cu B.Cu) (net 67))
  (segment (start 40.64 57.15) (end 40.64 77.47) (width 0.25) (layer F.Cu) (net 67))
  (segment (start 22.86 76.2) (end 20.32 76.2) (width 0.25) (layer B.Cu) (net 67))
  (segment (start 40.64 77.47) (end 24.13 77.47) (width 0.25) (layer B.Cu) (net 67))
  (segment (start 24.13 77.47) (end 22.86 76.2) (width 0.25) (layer B.Cu) (net 67))
  (segment (start 19.05 68.58) (end 20.32 68.58) (width 0.25) (layer B.Cu) (net 68))
  (segment (start 27.94 38.1) (end 26.67 36.83) (width 0.25) (layer B.Cu) (net 68))
  (segment (start 35.2679 38.1) (end 27.94 38.1) (width 0.25) (layer B.Cu) (net 68))
  (segment (start 26.67 36.83) (end 19.05 36.83) (width 0.25) (layer B.Cu) (net 68))
  (segment (start 19.05 36.83) (end 16.51 39.37) (width 0.25) (layer B.Cu) (net 68))
  (segment (start 16.51 39.37) (end 16.51 66.04) (width 0.25) (layer B.Cu) (net 68))
  (segment (start 16.51 66.04) (end 19.05 68.58) (width 0.25) (layer B.Cu) (net 68))
  (segment (start 21.44501 67.16501) (end 43.32499 67.16501) (width 0.25) (layer B.Cu) (net 70))
  (segment (start 20.32 66.04) (end 21.44501 67.16501) (width 0.25) (layer B.Cu) (net 70))
  (segment (start 44.45 66.04) (end 53.34 66.04) (width 0.25) (layer B.Cu) (net 70))
  (segment (start 43.32499 67.16501) (end 44.45 66.04) (width 0.25) (layer B.Cu) (net 70))

)
