(module SW_TH_DPDT_Pushbutton_Latched (layer F.Cu) (tedit 6066BDE4)
  (fp_text reference SW54 (at 0 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CAPSLK (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4 2) (end 4 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 4 2) (end 4 10) (layer F.SilkS) (width 0.12))
  (fp_line (start 4 10) (end -4 10) (layer F.SilkS) (width 0.12))
  (fp_line (start -4 10) (end -4 2) (layer F.SilkS) (width 0.12))
  (pad 5 thru_hole circle (at 2.54 3.429) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 2.54 5.969) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 2.54 8.509) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -2.54 8.509) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -2.54 5.969) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.54 3.429) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
)
